key:string|weight:string|sk:string|en:string
+|switching_profile_point_applied_to_line|INFORMATIONAL|Aplikovaný bod spínacieho profilu na línií č. ${line} : ${value}|Switching profile point applied to line no. ${line} : ${value}|...............
+|dusk_has_occured|INFORMATIONAL|Nastal súmrak: ${value}|Dusk has occured: ${value}|...............
+|dawn_has_occured|INFORMATIONAL|Nastal úsvit: ${value}|Dawn has occured: ${value}|...............
+|dimming_profile_was_successfully_received_by_node|NOTICE|Stmievací profil bol úspešne prijatý nodom č. ${node}|Dimming profile was successfully received by node no. ${node}|...............
+|master_node_is_responding_again|NOTICE|Master node začal znovu odpovedať|Master node is responding again|...............
+|command_was_sent_from_terminal_interface|DEBUG|Z terminálu bol odoslaný príkaz|A command was sent from terminal interface|...............
+|master_node_is_not_responding|ALERT|Master node neodpovedá|Master node is not responding|...............
+|configuration_of_dimming_profile_to_node_failed|ALERT|Konfigurácia stmievacieho profilu pre node č. ${node} zlyhala|Configuration of dimming profile to node no. ${node} has failed|...............
+|circuit_breaker_was_turned_on_line|NOTICE|Zapnutie ističa na línii č. ${line}|Circuit breaker was turned on - line no. ${line}|...............
+|circuit_breaker_was_turned_off_line|ERROR|Vypnutie ističa na línií č. ${line}|Circuit breaker was turned off - line no. ${line}|...............
+|dimming_profile_was_processed_for_node|INFORMATIONAL|Stmievací profil bol spracovaný pre node č. ${node}|Dimming profile was processed for node no. ${node}|...............
+|switching_profile_was_processed_for_line|INFORMATIONAL|Spínací profil bol spracovaný pre líniu č. ${line}|Switching profile was processed for line no.  ${line}|...............
+|thermometer_is_not_responding|WARNING|Teplomer neodpovedá|Thermometer is not responding|...............
+|thermometer_is_responding_again|NOTICE|Teplomer znovu odpovedá|Thermometer is responding again|...............
+|thermometer_sends_invalid_data|WARNING|Teplomer posiela neplatné hodnoty|Thermometer sends invalid data|...............
+|main_switch_has_been_turned_off|CRITICAL|Hlavný vypínač bol vypnutý|Main switch has been turned off|...............
+|main_switch_has_been_turned_on|NOTICE|Hlavný vypínač bol zapnutý|Main switch has been turned on|...............
+|power_supply_has_disconnected_input|ALERT|Napájací zdroj nemá napätie na vstupe|Power supply has disconnected input|...............
+|power_supply_works_correctly|NOTICE|Napájací zdroj pracuje správne|Power supply works correctly|...............
+|battery_level_is_low|ERROR|Batéria má nízku úroveň napätia|Battery level is low|...............
+|battery_level_is_ok|NOTICE|Batéria má správnu úroveň napätia|Battery level is OK|...............
+|door_main_open|NOTICE|Hlavné dvere boli otvorené|Main door has been opened|...............
+|door_em_open|NOTICE|Dvere silovej časti boli otvorené|Power door has been opened|...............
+|door_main_open_without_permission|WARNING|Hlavné dvere boli otvorené bez povolenia - zapnutá siréna|Main door has been opened without permission - alarm is on|...............
+|door_em_open_without_permission|WARNING|Dvere silovej časti boli otvorené bez povolenia|Power door has been opened without permission|...............
+|door_main_close|NOTICE|Hlavné dvere boli zatvorené|Main door has been closed|...............
+|door_em_close|NOTICE|Dvere silovej časti boli zatvorené|Power door has been closed|...............
+|state_of_contactor_for_line|INFORMATIONAL|Stav stýkača pre líniu č. ${line} je ${value}|State of contactor for line no. ${line} is ${value}|...............
+|local_database_is_corrupted|CRITICAL|||...............
+|electrometer_nok|ERROR|Elektromer neodpovedá|Electrometer is not responding|...............
+|electrometer_ok|NOTICE|Elektromer znovu odpovedá|Electrometer is responding again|...............
+|no_voltage_on_phase|CRITICAL|Na fáze č. ${phase} nie je napätie|No voltage detected on phase no. ${phase}|...............
+|voltage_on_phase_restored|NOTICE|Napätie na fáze č. ${phase} bolo obnovené|Voltage on phase no. ${phase} has been restored|...............
+|flow_start|NOTICE|FLOW bol spustený|FLOW has been started |...............
+|twilight_sensor_nok|ERROR|Sensor súmraku neodpovedá|Twilight sensor is not responding|...............
+|twilight_sensor_ok|NOTICE|Sensor súmraku znovu odpovedá|Twilight sensor is responding again|...............
+|lamps_have_turned_on|NOTICE|Lampy sa zapli|Lamps have turned on|...............
+|lamps_have_turned_off|NOTICE|Lampy sa vypli|Lamps have turned off|...............
+|flow_restart|NOTICE|FLOW bol reštartovaný|FLOW has been restarted|...............
+|nodes_db_changed|NOTICE|Zmena v node databáze|Node db has changed|...............
